Progress Fathom Replication
Installation Guide

> ## Replication server and agent ping

> If no message is received from the agent for a specified interval, the Replication server sends a ping message to the agent. Likewise, the agent pings the server if there has been no communication during a specified interval. If there is no response to the ping, the component that sent the ping assumes the connection is broken and begins failure recovery.

Copyright © 2004 Progress Software Corporation www.progress.com Voice: (781) 280-4000 Fax: (781) 280-4095